Republic of North Macedonia

Ministry of Transport and Communications

## Western Balkans Trade and Transport Facilitation Project

## AMENDMENT NO. 2

## To the Request for Bids for the procurement of

## Provision of customs related equipment - CCTV and ANPR systems –

##  installation, commissioning and training of Custom Administration staff

## Ref. No.: WBTTFP-8929-MK-121E-RFB

Issued on date: April 27, 2023

To all prospective Suppliers and to all firms that have obtained the RFB documents

Dear All,

With reference to the stated project and pursuant to the issued Request for Bids (RFB) for procurement of the above stated subject, please be informed of the following:

**1.** The relevant Clause of the RFB - Section II - Bid Data Sheet (BDS) - C. Preparation of Bids:

**ITB 15.1 is amended and now reads as follow:**

|  |  |
| --- | --- |
| **ITB 15.1**  | The Bidder **is not** required to quote in the currency of the Purchaser’s Country the portion of the Bid price that corresponds to expenditures incurred in that currency.In case that awarded Bidder (single bidder or JV lead member) is company registered in North Macedonia and bank account is in North Macedonia, the currency of the Contract Price shall be Macedonian denar (MKD) in accordance with national legislative. Due to this, if the awarded Bidder expressed Bid Price in any other currency, the Bid Price will be convert using the **buying** exchange rate in MKD and that amount in MKD will be Contract Price. **The Contract will be signed with Contract Price in MKD.** All amounts from payment schedule will be also convert in MKD and invoiced in MKD. All payments will be in MKD.The source of exchange rate shall be: National Bank of the Republic of North Macedonia The date for the exchange rate shall be*:* same as deadline for submission of the Bids. |

**2.** The relevant Clause of the RFB - Section VII – Schedule of Requirements - Detailed Technical Specifications - Required and Offered - **Position no. 20 – Monitor**

**is amended and now reads as follow:**

|  |  |
| --- | --- |
| **20** | **Monitor – Quantity 4 pcs** |
|  | * 1. Screen size 55 inch
	2. Resolution minimum 3840x2160 at 60 Hz
	3. At least two (2) HDMI interfaces
	4. **At least one (1) VGA interfaces**
	5. Power supply 220 VAC
 |

**3.** The relevant Clause of the RFB - Section VII – Schedule of Requirements - Detailed Technical Specifications - Required and Offered - **Position no. 23 - Network Switch**

**is amended and now reads as follow:**

|  |  |
| --- | --- |
| **23** | **Network Switch – Quantity 33 pcs** |
|  | * 1. At least twenty four (24) Gbps PoE network interface
	2. At least two (2) Gps fiber optical network interface
	3. Network topology management
	4. Alarm push
	5. Network health monitor
	6. PoE watchdog to auto detect and restart the cameras that do not respond
	7. Support of Layer 2 management protocols, STP/RSTP, VLAN, link aggregation, SNMP, QoS
	8. **At least hundred (100) meters PoE functionality**
	9. PoE watchdog functionality
	10. Fully compatible with the central software application
	11. 6 KV surge protection on PoE ports.
	12. Power supply
	13. **Working range temperature from -10 ° C to +50 ° C**
 |

**All other terms and conditions indicated in the issued RFB and issued Amendments no.1 and no.2 remain unchanged.**

**Please note that confirmation by e-mail of the receipt of this Amendment no.3 is compulsory!**

Yours sincerely,

**Slavko Micevski**

Procurement officer

*Western Balkans Trade and Transport Facilitation Project*

*Local Roads Connectivity Project*

*T: +38975494977*

*E:* *slavko.micevski.piu@mtc.gov.mk*

*Ministry of Transport and Communications*

*Crvena Skopska Opstina 4, 1000 Skopje
Republic of North Macedonia*

[*www.mtc.gov.mk*](http://www.mtc.gov.mk/)